**58MM Thermal Printer**

(Model No.: OCPP-58Z)

**Feature:**

* Small size and elegant design
* Can drive cash drawer
* The built-in power adapter
* Suport Android system
* Bar code printing funtion(optional)
* Compatible with ESPON
* Printing head life: 50KM

**Specification:**

|  |  |
| --- | --- |
| **Printing Method** | Direct thermal |
| **Print Density** | 384dots/line (203DPI) |
| **Character Size** | 384dots/line, ANK character, Font: A: 12\*24dots, 1.5(W)\*3.0(H) mm  Simplified/Traditional: 24\*24dots, 3.0(W)\*3.0(H)mm |
| **Barcode Type** | JAN13(EAN13) JAN8(EAN8) CODE39 |
| **Printing Command** | Compatible with EPSON ESC/POS |
| **Language** | Buyer language support |
| **Printing Speed** | 90mm/sec(max) |
| **Paper Width** | 57.5±0.5mm |
| **Paper Thickness** | 0.06-0.08mm |
| **MCBF(life)** | 50km |
| **Dimension** | 175\*130\*110mm |
| **Gross Weight** | 0.8 KG |
| **Auto Cutter** | manual cutter |
| **Sensor** | Paper Near End Sensor, Paper End Sensor, Cover open sensor |
| **Roll Paper** | Φ75mm |
| **Interface** | USB |
| **Driver** | Win 9X, Win 2000, Win 2003, Win XP, Win Vista, Win 7,Win8 compatible with ESPON |
| **Adapter Voltage Input** | AC 110V/220V, 50-60Hz |
| **Adapter Voltage Output** | DC12V/3A |
| **Printer Input Voltage** | DC12V/3A |
| **Cash Drawer Control** | DC12V/1A |
| **Working Temperature** | 0-45degree C, Humidity: 10-80% |
| **Saving Temperature** | -10-60degree C, Humidity: 10-90% |
| **Certificate** | CE/FCC/CCC/RoHS |